This is the scope when I sent the character "ctrl+a" which corresponds to ASCII code 00000001 in binary. In the UART protocol, start bits are low and begin with the least significant bit. This is reflected in the scope since it is apparent the signal began with a low portion (the start bit) and then went high for a single bit length. 