In order to connect the FPGA to an oscilloscope as I was instructed to do, I connected a female jumper wire to the pin 40 on the serial port connection that was found on the FPGA. I then connected the ground of the probe to the ground on the audio port. 